Product Information

Product Name: Gray Masterbatch

Product Code: 01-1260-03

Carrier Resin: PE

Masterbatch Type: Opaque

Proper to use in: PE- PP

Description: Gray Masterbatch is designed to mix with Polyethylene and Polypropylene to use for injection molding, blow molding and… .

Benefits: It’ll be completely solved in polymer. When the granules are mixed with polymer matrix and it has been molded, the final production has bright gray color.

Technical Data

Heat Stability: 240°C

Use this masterbatch in 1% of weight.

Gray masterbatch includes mineral filler.

Keep this product in dry place below 40° Centigrade

Tel: 021-56572878-9 [www.payonpolymer.com](http://www.payonpolymer.com)

Tel fax: 021-56572880 info@[www.payonpolymer.com](http://www.payonpolymer.com)